T. Weidberg SCT Links Meeting, 18th Feburrary ‘99.

Dog-leg to Low Mass Tape Connection

•System test 98 used ZIF connector to join dog-leg to Al power tape. •ATLAS solution should a void connectors

- minis mass - reliability

•Solder connection

Al tapes (single sided)

Cu dog-leg (double sided)

Bridge

solder

T. Weidberg SCT Links Meeting, 18th Feburrary ‘99.

•Operation

- apply solder with “silk scr een” pr ocess - attach with temporary tape. - apply heat with hot air blower (will pur chase special hot air blower for SMD work) and r emove tape.

•Examples

- Double sided Cu to single sided Cu connection. - single sided Al to Cu connection. - n.b. Al requir es Ni/Au plating (can be done by Ljubljana). - Cu tape can also be Ni/A u plated.