T. Weidberg SCT Links Meeting, 18th Feburrary ‘99.

New Soruces for Opto-packges

•Honeywell.

- Common de velopment with CMS (P eter Denes). CMS ECAL r equir es 80,000 VCSELs. - Based on surface mount VCSEL package(==> Figur e) - Use angle cut and polished fibr e to couple light from VCSEL into fibr e. - Use 3013 PIN diode in similar package. Already tested f or radiation hardness. - First pr ototype of VCSEL only will be common development with CMS (==> Figur e). - Next stage would be ATLAS SCT pr ototype (2 VCSELs and one PIN).

T. Weidberg SCT Links Meeting, 18th Feburrary ‘99.

•Ohio State Uni versity - simple package based on machined ceramic. - VCSELs mounted on end of ceramic. - fibr es in separate ceramic using taper ed holes. - Passive alignment of tw o parts (==> Figur e). - First tests with packages in Mar ch. - Produce VCSEL/PIN package. - Production in-house or in industry ?

•Truelight

- Inter ested in off-detector arrays. - Possible inter est in on-detector packages.