CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

StAF Architecture Standard Analaysis Framework

Craig E. Tull NERSC - LBNL ATLAS Software Week CERN May 20, 1999

HENP Computing Challenges

Experiment Data Compute

E895 (AGS) 10 TB/yr 600 SPECint95

BaBar (SLAC) 400 TB/yr 5,000 SPECint95

STAR (RHIC) 266 TB/yr 10,100 SPECint95

PHENIX (RHIC) 700 TB/yr 8,500 SPECint95

D0 Run II (FNAL) 280 TB/yr 4,075 SPECint95

CDF Run II (FNAL) 464 TB/yr 3,650 SPECint95

ATLAS (LHC) 1100 TB/yr 2,000,000 SPECint95

Experiment Contries Institutes Collaborators Time Frame

E895 (AGS) 3 12 49 2000

BaBar (SLAC) 9 85 600 2010

STAR (RHIC) 7 3 400 2010

PHENIX (RHIC) 10 41 400 2010

D0 Run II (FNAL) 11 77 500 2005

CDF Run II (FNAL) 8 41 490 2005

ATLAS (LHC) 34 144 1700 2015

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

What is a Framework?

� Gamma, et al., Design Patterns

"When you use a toolkit, you write the main body of the application and call the code you want to reuse. When you use a framework, you reuse the main body and write the code it calls."

"Not only can you build applications faster as a result, but the applications have similar structures. They are easier to maintain, and they seem more consistent to their users. On the other hand, you lose some creative freedom, since many design decisions have been made for you."

"If applications are hard to design, and toolkits are harder, then frameworks are hardest of all. ... Any substantive change to the framework’s design would reduce its benefits considerably, since the framework’s main contribution to an application is the architecture it defines. Therefore it’s imperative to design the framework to be as flexible and extensible as possible."

StAF Design Features

� Horizontal AND Vertical Modularity

� TRUE Component Software

� Components go in AND out

� Explicit graceful retirement

� Adoption or imitation of industry standards

� Scripting access to underlying code API

� Reliance on code & doc generation tools

� stic, SWIG, idldoc, stafgen, pamigen, Orbix idl

� Dynamic Linking & Unlinking of Components

� Multi-language support

� Legacy software (& larger FTE pool)

� N.B. C++ will be a legacy language before 2015

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

Software Bus & Modularity

� �Horizontal Mod.� reflects ASP domains (ie. functionality). � �Vertical Mod.� reflects protocol & interface standards. � CORBA provides a well defined interface standard, a fully functional software bus, & auto. Client-Server capability.

� SOC - Collocated Software Bus ASP

� Gateway to real ORB

User Interface (eg. KUIP, Tcl, � ) Command Marshalling (eg. *_def.cdf, swig)

ASP C++ Classes/Objects

Software Bus (eg. CORBA, SOC)

StAF Architecture

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

CORBA

� Non-Proprietary Software Bus Specification � Object Oriented Client-Server Architecture � Distributed Computing

� Location Transparency � Heterogeneous, distributed environment � Event Granularity ⇒ Event Farming � Information flow between processes � Data Table - large & simple (XDR-opaque) � Control Messages - small & complex � IDL - Interface Definition Language � Purely descriptive -- No operations � Syntax & scoping similar to C++

STAF Objects & Packages

� ASP - Object Factories (singletons)

� create/find/delete worker objects

� ASP - Worker Objects

� C++ classes to do system-like work of FW

� PAM - Calculation Objects

� C++ classes for user-written algorithmic code

� Data Objects

� Tables: smart structs (run-time type checking, etc.)

� Datasets: containers (UNIX FS-like hierarchy)

� Error Stack - ASPs & PAMs condition values

� Result Stack - queried attribute values & scratch

Analysis Service Package

� CORBA-compliant C++ class library � 1 Object Factory Class (singleton) � 0 or more Worker Object Classes � Communication & Control � Software Bus � Serves a single purpose or set of purposes � System-like Services (I/O, Mem mgt, DB, etc.)

� Normally independent of other ASPs � Limited interdependency realizable � Can be statically or dynamically linked � Generic - not specific to data table types � Directly available from UI, CORBA, or code

Object Factories

� Factory Attributes/Methods

readonly attribute long count;

  - Count of manufactured objects

STAFCV_T list();

  - Method to list manufactured objects

� Methods for each worker class (eg. thing)

thing* newThing(in TYPE ARGUMENT, ...);

  - Construct a new thing object
thing* findThing(in string SORef);

  - Find the thing object specified by SORef

STAFCV_T deleteThing(in string SORef);

  - Destruct the thing object specified by

  SORef (Stringified Object Reference)

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

IDL in StAF

� defining table types

IDL              Ansi-C/C++       FORTRAN
short            short            INTEGER*2
long             long             INTEGER*4
char             char             CHARACTER*1
float            float            REAL*4

� scalars, vectors, arrays, structs � defining analysis module interfaces (type 1 API)

� interface

� Define analysis module interface

� in, out, inout

� Define I/O mode for table arguments to module

� defining service package interfaces

� Fuller subset of IDL usable

stic - STAR IDL Compiler

� Automates many user tasks

� Eases learning curve

� Enforces consistency w/ architecture

� Speeds development

� Dataset Tables

� Automatic generation of .h & .inc files

� Physics Analysis Modules

� Automatic generation of interface code

� Generation of PAM skeleton code

� Automatic generation of life-cycle code

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

stic - usage

� lex & yacc based IDL compiler - H.Ward

Usage: ./stic [-h?rMTivftq] [-Iincdir] [-static|-dynamic] [xxx.idl]

-? Prints this usage message and then immediately quit.
-dynamic Dynamic tables.
-f Produce only header files (.h and .inc).
-h Prints this usage message and then immediately quit.
-H Produce only the header   files.
-i Ignore case (upper converted to lower).
-I Mechanism for specifying list of include directories.
-M Write string to stdout for use in a Makefile, no other output.
-T Write string with used tables to stdout for use in a Makefile, no
   other output.
-q Operate quietly.
-static  Static tables.
-t Produce only the template files.
-r Produce only the ROOT files.
-v Write version info to stdout, no other output is produced.

User Code - Analysis Modules

� User-written physics code (F77, C, C++)

� Interface defined by IDL

� interface findv:amiModule{

  STAFCV_T call(inout part p, out event ev);};

� Callable from user interface

� KUIP> MODULE/CALL findv part evt

� Access to data as program variables

� INTEGER*4 FUNCTION FINDV(P_H, P, EV_H, EV)

  DS2REALLOCTABLE(EV_H,EV,P_H.NOK) ! reallocate

  table memory

  EV_H.NOK = 1

  EV(1).MULTIPLICITY = P_H.NOK

  DO I=1,P_H.NOK

   EV(1).MAX_Z = MAX(P(I).Z,EV(1).MAX_Z)

  ENDDO

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

DSL - Datasets & Tables

� Self-Describing Machine Independent Data Format based on Sun�s XDR & CORBA IDL � disk, tape, network, other � AIX, HP-UX, IRIX, Linux, OSF1, SunOS 4.x, Solaris 2.x, Solaris X86, CRAY T3E, Windows � Complex Data Types & Hierarchic Datasets � directed acyclic graphs � Low overhead & high performance � Dynamic Memory Allocation � Random Access (Table = atomic data unit) � C++ Class Library (100% consistent with C API) � RDB Functions (Join, Project)

Unix-like Dataset Hierarchy

� SAMPLE

   *****************************************************

   EVENT---+CONFIG-+Run                                   *

           |       |                                      *

           |       +CALIB---...                           *

           |                                              *

           +RAW----+TPC----+SECT01-+Sequence              *

           |       |       |       |                      *

           |       |       |       +Data                  *

           |       |       ...                            *

           |       |       |                              *

           |       |       +SECT24-+Sequence              *

           |       |               |                      *

           |       |               +Data                  *

   ********************************************************

� Unix-like commands.

� cd, cp, ln, ls, mkdir, mv, pwd, rm, rmdir

� Data are logically organized by hierarchy.

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

StAF User Interface

� Interface layered for �Graceful Retirement� � Scripting Language vs. GUI

� More control/programmability (GUI second) � Current interface implemented by KUIP � Fully functional Tcl interface implemented - DP � Interface reflects underlying classes

� Maximum control at user interface level � Less transition penalty between languages

C++ dioFileStream * oldat = dio->newFileStream("oldat","old_data.xdf","R");

oldat->getEvent("."); KUIP DIO/NEWFILESTREAM oldat old_data.xdf R

GETEVENT olddat . Tcl dio newFileStream oldat old_data.xdf R

oldat getEvent .

The right tool for the job

� Programming languages are designed for building data struct.s & algorithms from scratch.

� strongly typed to manage complexity

� Scripting languages are designed for gluing applications.

� higher level of programming

� more rapid application development

� programmers write same # of LOC per year

� programmable applications (User Interface)

� trade off execution efficiency for devel’t speed

� computers are getting faster

� FORTRAN & ALGOL vs Assembler in early 60s

KUIP StAF Interface

Tcl StAF Interface

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

StAF Table Broswer

Tcl/Tk BLT Tree Tool

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

StAF ASPs & PAMs

� AMI - Analysis Module

Invoker � DIO - Dataset Input/Output � DUI - Dataset Unix-like

Interface � EML - Error Messaging & Logging � GCA - Grand Challenge Archictecture � ISS - DPSS Input/Output � LEV - Logging of

Environment & Versions � NIO - Ntuple Input/Output � OIO - Objectivity Input/Output (non-functional) � PIO - PHENIX Input/Output

� RDB - Relational (Oracle) Database � RTI - Root Table Interface � SOC - Service & Object Catalog � SPX - Service Package eXample � TBR - Motif Table BRowser � TDM - Table & Dataset Memory � TNT - Table to NTuple � TOP - Table RDB OPerators

� STAR Analysis pre-MDC1 � 400 Tables � 150 PAMs

StAF OS Coverage

� StAF has successfully built and run on:

� AIX, HP-UX, IRIX, Linux, OSF1, SunOS 4.x,

Solaris 2.x, Solaris X86, CRAY T3E, Windows

NT 4, Windows 95

� Current state of makefiles

� AIX, IRIX, Linux, Solaris 2.x (egcs, CC 4.2, CC

5.0 w/ -compat=4)

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

Projects Using StAF

� STAR

� Most physics SW development � Successful MDC1 � PHENIX

� MDC1 & MDC2 � E896 (AGS)

� 1.4 M real events analyized � Grand Challenge

� First development & deployment platform � Clipper

� Wide Area Scientific Data Access project � 35 MB/sec I/O between SLAC & LBNL

ATLAS - Analysis Framework

� Data Analysis Framework-"like" Programs

� ac++, arve, basis, cleo, d0 fw, dspack, gaudi, jas, lulu, openscientist, paw, root, staf, tas, ...

� Publicly Available Tools & Technologies

� ace, coool, corba, ddl, grdoc, idl, idldoc, ilu, java, javacc, jini, mysql, netlogger, odl/oif, python, sun idl-cfe, swig, tcl, tk, uml/xmi, ...

� ATLAS Framework must be in place EARLY (now)

& LONG (~20 years!).

� Challenge: Allow adoption of technologies unknown at time of 1st version of FW.

CETull@lbl.gov : ATLAS SW Week : 20may99 : http://iago.lbl.gov/

SLAC ⇒ LBL -- DPSS Write Test

SLAC ⇐ LBL -- DPSS Read Test